NOTES:
· dimensions specified in cm,
· cover of bottom reinforcement bars 7 cm
· connect foundations to the lightning conductor according to the industry drawings
· place the prefabricated foundation on a levelled substrate (sand and gravel bed 30 cm thick compacted Id = 0.8)
· in the case of pouring the foundation slab on site, do not make the assembly rod No. 3
· maximum substrate pressure does not exceed 90 kPa
CONCRETE B-25
STEEL A-III
no.
no.
no.
no.
no.
FOUNDATION F-1
scale 1:20
no.
no.
no.
no.
no.
sand and gravel bed 30 cm thick
no.
no.
sand and gravel bed 30 cm thick
no.
no.
no.
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